### Installation

The Beijer Exter T70-bl comes with a standard software version that needs to be changed to a proprietary version.

To install the software, the following steps have to be made

#### Boot the Exter T70 system

The system automatically boots when the power is connected.

#### Connect the Exter T70 to the maintenance PC

Using a cross-over cable between the PC and Exter T70 panel or a straight-cable

between a network switch and the PC and the network switch and the panel.

*: be sure that only one uninitialized Exter T70 panel is connected to your network to prevent IP conflicts.*

#### Check the IP address of the maintenance PC

The IP address of the maintenance PC should be in the same subnet as the Exter T70.

Default settings of the Exter T70: IP: 192.168.1.1, Subnet-Mask: 255.255.0.0.

#### Copy the new software

To do this, open Windows Explorer and go to the local copy of the Alarm Panel

Software (to be found at Sharepoint). Select the folder “NavVisionUpdate” and click right mouse button and select

“Copy”

*:Make sure you use the right version for the BNWAS setup. At least the version of DisplayServer.exe needs to be 2.0*

*:The NavVision software version needs to be 9.18.4.100 or higher.*




Figure 2‑7: Copy local files

#### Open an FTP connection to the Exter T70 panel.

You can do this by opening Windows Explorer and entering the ftp address in the address

bar. By default it is: ftp://free:technics@192.168.1.1

Change the IP address by the assigned IP address in FT NavVision, when the Exter T70

was already initialized.




Figure 2‑8: Enter FTP address

#### Paste the files you have just copied

To do this, press right mouse button and select “Paste”




Figure 2‑9: Paste new files

#### Activating update

The panel will automatically update, when it is the first time the software is installed on the

Exter T70. When it’s an update of the Exter T70, the power to the unit should be turned off

and on again.